This is a copy of one node from the Info file gcc.info-3.
For full information on installing and porting GCC, refer to the
GCC manual:

  Info file   gcc.info
  TeX output  gcc.dvi
  TeX source  gcc.texinfo

Installing GNU CC
*****************

   Here is the procedure for installing GNU CC on a Unix system.

* Menu:

* Other Dir::     Compiling in a separate directory (not where the source is).
* Sun Install::   See below for installation on the Sun.
* 3B1 Install::   See below for installation on the 3B1.
* SCO Install::   See below for installation on SCO System V 3.2.  (Or ESIX.)
* VMS Install::   See below for installation on VMS.
* HPUX Install::  See below for installation on HPUX.
* Tower Install:: See below for installation on an NCR Tower.

  1. Edit `Makefile'.  If you are using HPUX, or any form of system V,
     you must make a few changes described in comments at the beginning
     of the file.  Genix requires changes also, and so does the Pyramid.

  2. On a Sequent system, go to the Berkeley universe.

  3. Choose configuration files.  The easy way to do this is to run the
     command file `config.gcc' with a single argument, which specifies
     the type of machine (and in some cases which operating system).

     Here is a list of the possible arguments:

    `vax'
          Vaxes running BSD.

    `vms'
          Vaxes running VMS.

    `vax-sysv'
          Vaxes running system V.

    `i386-sysv'
          Intel 386 PCs running system V.

    `i386-sysv-gas'
          Intel 386 PCs running system V, using the GNU assembler and
          GNU linker.

    `i386-sysv4'
          Intel 386 PCs running system V.4.  You must run the shell
          script `fixincludes-V4' in order for GNU CC to work properly.
           You must also uncomment some lines in `Makefile'.

    `sequent-i386'
          Sequent with Intel 386 processors.

    `i386-aix'
          Intel 386 PCs or PS/2s running AIX.

    `sun2'
          Sun 2 running system version 2 or 3.

    `sun3'
          Sun 3 running system version 4, with 68881. Note there we do
          not provide a configuration file to use an FPA by default,
          because programs that establish signal handlers for floating
          point traps inherently cannot work with the FPA.

    `sun3-nfp'
          Sun 3 running system version 4, without 68881.

    `sun4'
          Sun 4 running system version 4.  *Note Incompatibilities::,
          for calling convention incompatibilities on the Sun 4 (sparc).

    `sun2-os4'
          Sun 2 running system version 4.

    `sun3-os3'
          Sun 3 running system version 2 or 3, with 68881.

    `sun3-nfp-os3'
          Sun 3 running system version 2 or 3, without 68881.

    `sun4-os3'
          Sun 4 running system version 2 or 3.  *Note
          Incompatibilities::, for calling convention incompatibilities
          on the Sun 4 (sparc).

    `sun386'
          Sun 386 ("roadrunner").

    `alliant'
          Alliant FX/8 computer.  Note that the standard installed C
          compiler in Concentrix 5.0 has a bug which prevent it from
          compiling GNU CC correctly.  You can patch the compiler bug
          as follows:

               cp /bin/pcc ./pcc
               adb -w ./pcc - << EOF
               15f6?w 6610
               EOF

          Then you must use the `-ip12' option when compiling GNU CC
          with the patched compiler, as shown here:

               make CC="./pcc -ip12" CFLAGS=-w

          Note also that Alliant's version of DBX does not manage to
          work with the output from GNU CC.

    `tahoe'
          The tahoe computer (running BSD, and using DBX).

    `decstation'
          The DEC 3100 Mips machine ("pmax").  Note that GNU CC cannot
          generate debugging information in the unusual format used on
          the Mips.

    `mips-sysv-os5'
          The Mips computer, RS series, with the System V environment
          running on revision 5.00 of RISC-OS as default. Note that GNU
          CC cannot generate debugging information in the unusual
          format used on the Mips, and also cannot be used to create
          programs that use shared libraries.

    `mips-sysv'
          The Mips computer, RS series, with the System V environment
          as default. Note that GNU CC cannot generate debugging
          information in the unusual format used on the Mips.

    `mips-bsd43-os5'
          The Mips computer, RS series, with the BSD 4.3 environment
          running revision 5.00 of RISC-OS as default. Note that GNU CC
          cannot generate debugging information in the unusual format
          used on the Mips, and also cannot be used to create programs
          that use shared libraries.

    `mips-bsd43'
          The Mips computer, RS series, with the BSD 4.3 environment as
          default. Note that GNU CC cannot generate debugging
          information in the unusual format used on the Mips.

    `mips-os5'
          The Mips computer, M series running revision 5.00 of RISC-OS.
          Note that GNU CC cannot generate debugging information in the
          unusual format used on the Mips, and also cannot be used to
          create programs that use shared libraries.

    `mips'
          The Mips computer, M series.  Note that GNU CC cannot
          generate debugging information in the unusual format used on
          the Mips.

    `iris'
          Another variant of the Mips computer, the Silicon Graphics
          Iris 4D. Note that GNU CC cannot generate debugging
          information in the unusual format used on the Mips.

    `convex-c1'
          Convex C1 computer.  With operating system version 9, use `cc
          -pcc' as the compilation command when building stage 1 of GNU
          CC.

    `convex-c2'
          Convex C2 computer.  With operating system version 9, use `cc
          -pcc' as the compilation command when building stage 1 of GNU
          CC.

    `pyramid'
          Pyramid computer.

    `hp9k320'
          HP 9000 series 300 using HPUX assembler.  Note there is no
          support in GNU CC for HP's debugger; thus, `-g' is not
          available in this configuration.

    `hp9k320-gas'
          HP 9000 series 300 using GNU assembler, linker and debugger.
          This requires the HP-adapt package, which is available along
          with the GNU linker as part of the "binutils" distribution.
          This is on the GNU CC distribution tape.

    `hp9k320-old'
          HP 9000 series 300 using HPUX assembler, in operating system
          versions older than 6.5.  Note there is no support in GNU CC
          for HP's debugger; thus, `-g' is not available in this
          configuration.

    `hp9k320-bsd'
          HP 9000 series 300 running BSD.

    `hp9k200-bsd'
          HP 9000 series 200 running BSD.  Note that the C compiler
          that comes with this system cannot compile GNU CC; contact
          `law@super.org' to get binaries of GNU CC for bootstrapping. 
          Additionally, a minor patch is necessary if you wish to build
          kernels with GNU CC; contact `law@super.org' to get a copy of
          the patch.

    `isi68'
          ISI 68000 or 68020 system with a 68881.

    `isi68-nfp'
          ISI 68000 or 68020 system without a 68881.

    `news800'
          Sony NEWS 68020 system.

    `next'
          NeXT system.

    `tower'
          NCR Tower 32 system.

    `altos'
          Altos 3068.  Note that you must use the GNU assembler, linker
          and debugger, with COFF-encapsulation.  Also, you must fix a
          kernel bug.  Details in the file `ALTOS-README'.

    `3b1'
          AT&T 3b1, a.k.a. 7300 PC.  Note that special procedures are
          needed to compile GNU CC with this machine's standard C
          compiler, due to bugs in that compiler.  *Note 3b1 Install::.
           You can bootstrap it more easily with previous versions of
          GNU CC if you have them.

    `3b1-gas'
          AT&T 3b1 using the GNU assembler.

    `sequent-ns32k'
          Sequent containing ns32000 processors.

    `encore'
          Encore ns32000 system.

    `genix'
          National Semiconductor ns32000 system.

    `88000'
          Motorola 88000 processor.  This port is not finished.

     Here we spell out what files need to be set up:

        * Make a symbolic link named `config.h' to the top-level config
          file for the machine you are using (*note Config::.).  This
          file is responsible for defining information about the host
          machine.  It includes `tm.h'.

          The file is located in the subdirectory `config'.  Its name
          should be `xm-MACHINE.h', with these exceptions:

         `xm-vms.h'
               for vaxen running VMS.

         `xm-vaxv.h'
               for vaxen running system V.

         `xm-i386v.h'
               for Intel 80386's running system V.

         `xm-sun386i.h'
               for Sun roadrunner running any version of the operating
               system.

         `xm-hp9k320.h'
               for the HP 9000 series 300.

         `xm-genix.h'
               for the ns32000 running Genix

          If your system does not support symbolic links, you might
          want to set up `config.h' to contain a `#include' command
          which refers to the appropriate file.

        * Make a symbolic link named `tm.h' to the machine-description
          macro file for your machine.  It should be in the subdirectory
          `config' and its name should be `tm-MACHINE.h'.

          If your system is a 68000, don't use the file `tm-m68k.h'
          directly.  Instead, use one of these files:

         `tm-sun3.h'
               for Sun 3 machines with 68881.

         `tm-sun3-nfp.h'
               for Sun 3 machines with no hardware floating point.

         `tm-sun3os3.h'
               for Sun 3 machines with 68881, running Sunos version 3.

         `tm-sun3os3nf.h'
               for Sun 3 machines with no hardware floating point,
               running Sunos version 3.

         `tm-sun2.h'
               for Sun 2 machines.

         `tm-3b1.h'
               for AT&T 3b1 (aka 7300 Unix PC).

         `tm-isi68.h'
               for Integrated Solutions systems.  This file assumes you
               use the GNU assembler.

         `tm-isi68-nfp.h'
               for Integrated Solutions systems without a 68881.  This
               file assumes you use the GNU assembler.

         `tm-news800.h'
               for Sony NEWS systems.

         `tm-hp9k320.h'
               for HPUX systems, if you are using GNU CC with the
               system's assembler and linker.

         `tm-hp9k320g.h'
               for HPUX systems, if you are using the GNU assembler,
               linker and other utilities.  Not all of the pieces of
               GNU software needed for this mode of operation are as
               yet in distribution; full instructions will appear here
               in the future.

         `tm-tower-as.h'
               for NCR Tower 32 systems, using the standard system
               assembler.

          For the vax, use `tm-vax.h' on BSD Unix, `tm-vaxv.h' on
          system V, or `tm-vms.h' on VMS.

          For the Motorola 88000, use `tm-m88k.h'.  The support for the
          88000 does not currently work; it requires extensive changes
          which we hope to reconcile in version 2.

          For the 80386, don't use `tm-i386.h' directly.  Use
          `tm-i386v.h' if the target machine is running system V,
          `tm-i386gas.h' if it is running system V but you are using the
          GNU assembler and linker, `tm-seq386.h' for a Sequent 386
          system, or `tm-compaq.h' for a Compaq, or `tm-sun386i.h' for
          a Sun 386 system.

          For the Mips computer, there are five choices: `tm-mips.h'
          for the M series, `tm-mips-bsd.h' for the RS series with BSD,
          `tm-mips-sysv.h' for the RS series with System V, `tm-iris.h'
          for the Iris version of the machine, and `tm-decstatn.h' for
          the Decstation.

          For the 32000, use `tm-sequent.h' if you are using a Sequent
          machine, or `tm-encore.h' for an Encore machine, or
          `tm-genix.h' if you are using Genix version 3; otherwise,
          perhaps `tm-ns32k.h' will work for you.

          Note that Genix has bugs in `alloca' and `malloc'; you must
          get the compiled versions of these from GNU Emacs and edit
          GNU CC's `Makefile' to use them.

          Note that Encore systems are supported only under BSD.

          For Sparc (Sun 4) machines, use `tm-sparc.h' with operating
          system version 4, and `tm-sun4os3.h' with system version 3.

          For Convex systems before version 8.1, use `tm-conv1os7.h' or
          `tm-conv2os7.h'.  For versions 8.1 and greater, use
          `tm-convex1.h' or `tm-convex2.h'.  You should also bootstrap
          GCC with `pcc' rather than `cc'; one way to do this is with
          the following commands.

               ln -s /bin/pcc ./cc
               set path = (. $path)

        * Make a symbolic link named `md' to the machine description
          pattern file.  It should be in the `config' subdirectory and
          its name should be `MACHINE.md'; but MACHINE is often not the
          same as the name used in the `tm.h' file because the `md'
          files are more general.

        * Make a symbolic link named `aux-output.c' to the output
          subroutine file for your machine.  It should be in the
          `config' subdirectory and its name should be `out-MACHINE.c'.

  4. Make sure the Bison parser generator is installed.  (This is
     unnecessary if the Bison output files `c-parse.tab.c' and `cexp.c'
     are more recent than `c-parse.y' and `cexp.y' and you do not plan
     to change the `.y' files.)

     Bison versions older than Sept 8, 1988 will produce incorrect
     output for `c-parse.tab.c'.

  5. If you have a previous version of GCC installed, then chances are
     you can compile the new version with that.  Do the following:

          make CC="gcc -O"

     Since this produces an optimized executable right away, there is
     no need to bootstrap the result with itself except to test it. 
     Therefore, you can skip directly to the `make install' step below.

  6. Build the compiler.  Just type `make' in the compiler directory.

     Ignore any warnings you may see about "statement not reached" in
     the `insn-emit.c'; they are normal.  Any other compilation errors
     may represent bugs in the port to your machine or operating
     system, and should be investigated and reported (*note Bugs::.).

     Some commercial compilers fail to compile GNU CC because they have
     bugs or limitations.  For example, the Microsoft compiler is said
     to run out of macro space.  Some Ultrix compilers run out of
     expression space; then you need to break up the statement where
     the problem happens.

  7. If you are using COFF-encapsulation, you must convert `gnulib' to
     a GNU-format library at this point.  See the file `README-ENCAP'
     in the directory containing the GNU binary file utilities, for
     directions.

  8. Move the first-stage object files and executables into a
     subdirectory with this command:

          make stage1

     The files are moved into a subdirectory named `stage1'. Once
     installation is complete, you may wish to delete these files with
     `rm -r stage1'.

  9. Recompile the compiler with itself, with this command:

          make CC=stage1/gcc CFLAGS="-g -O -Bstage1/"

     This is called making the stage 2 compiler.

     On a 68000 or 68020 system lacking floating point hardware, unless
     you have selected a `tm.h' file that expects by default that there
     is no such hardware, do this instead:

          make CC=stage1/gcc CFLAGS="-g -O -Bstage1/ -msoft-float"

 10. If you wish to test the compiler by compiling it with itself one
     more time, do this (in C shell):

          make stage2
          make CC=stage2/gcc CFLAGS="-g -O -Bstage2/"
          foreach file (*.o)
          cmp $file stage2/$file
          end

     This is called making the stage 3 compiler.  Aside from the `-B'
     option, the options should be the same as when you made the stage 2
     compiler.

     The `foreach' command (written in C shell) will notify you if any
     of these stage 3 object files differs from those of stage 2.  On
     BSD systems, any difference, no matter how innocuous, indicates
     that the stage 2 compiler has compiled GNU CC incorrectly, and is
     therefore a potentially serious bug which you should investigate
     and report (*note Bugs::.).

     On systems that use COFF object files, bytes 5 to 8 will always be
     different, since it is a timestamp.  On these systems, you can do
     the comparison as follows (in Bourne shell):

          for file in *.o; do
          echo $file
          tail +10c $file > foo1
          tail +10c stage2/$file > foo2
          cmp foo1 foo2
          done

     On MIPS machines, you should use the shell script `ecoff-cmp' to
     compare two object files.

 11. Install the compiler driver, the compiler's passes and run-time
     support. You can use the following command:

          make install

     On some machines, you will find that starts to recompile the `.c'
     files, due to a bug in Make.  If that happens, cancel it and try
     again specifying the same values for Make variables that you used
     in the last compilation; that may not prevent the spurious
     recompilation, but will at least do it properly.  For example:

          make CC=stage2/gcc CFLAGS="-g -O -Bstage2/" install

     The `install' target copies the files `cc1', `cpp' and `gnulib' to
     files `gcc-cc1', `gcc-cpp' and `gcc-gnulib' in directory
     `/usr/local/lib', which is where the compiler driver program looks
     for them.  It also copies the driver program `gcc' into the
     directory `/usr/local/bin', so that it appears in typical
     execution search paths.

     *Warning: there is a bug in `alloca' in the Sun library. To avoid
     this bug, install the binaries of GNU CC that were compiled by GNU
     CC.  They use `alloca' as a built-in function and never the one in
     the library.*

     *Warning: the GNU CPP may not work for `ioctl.h', `ttychars.h' and
     other system header files unless the `-traditional' option is
     used.*  The bug is in the header files: at least on some machines,
     they rely on behavior that is incompatible with ANSI C.  This
     behavior consists of substituting for macro argument names when
     they appear inside of character constants.  The `-traditional'
     option tells GNU CC to behave the way these headers expect.

     Because of this problem, you might prefer to configure GNU CC to
     use the system's own C preprocessor.  To do so, make the file
     `/usr/local/lib/gcc-cpp' a link to `/lib/cpp'.

     Alternatively, on Sun systems and 4.3BSD at least, you can correct
     the include files by running the shell script `fixincludes'.  This
     installs modified, corrected copies of the files `ioctl.h',
     `ttychars.h' and many others, in a special directory where only
     GNU CC will normally look for them.  This script will work on
     various systems because it chooses the files by searching all the
     system headers for the problem cases that we know about.

     Use the following command to do this:

          make includes

     If you selected a different directory for GNU CC installation when
     you installed it, by specifying the Make variable `prefix' or
     `libdir', specify it the same way in this command.

     Note that some systems are starting to come with ANSI C system
     header files.  On these systems, don't run `fixincludes'; it may
     not work, and is certainly not necessary.

     *Warning:* `fixincludes' does not work on many MIPS systems,
     because those systems come with circular symbolic links which cause
     `ls -lR' to go into an infinite loop.  The same problem may occur
     on some versions of SunOS.  If you encounter this problem, try
     using `fixinc.new' instead opf `fixincludes'.

   If you cannot install the compiler's passes and run-time support in
`/usr/local/lib', you can alternatively use the `-B' option to specify
a prefix by which they may be found.  The compiler concatenates the
prefix with the names  `cpp', `cc1' and `gnulib'. Thus, you can put the
files in a directory `/usr/foo/gcc' and specify `-B/usr/foo/gcc/' when
you run GNU CC.

   Also, you can specify an alternative default directory for these
files by setting the Make variable `libdir' when you make GNU CC.


File: gcc.info,  Node: Other Dir,  Next: Sun Install,  Prev: Installation,  Up: Installation

Compilation in a Separate Directory
===================================

   If you wish to build the object files and executables in a directory
other than the one containing the source files, here is what you must
do differently:

  1. Go to that directory before running `config.gcc':

          mkdir gcc-sun3
          cd gcc-sun3

     On systems that do not support symbolic links, this directory must
     be on the same file system as the source code directory.

  2. Specify where to find `config.gcc' when you run it:

          ../gcc-1.36/config.gcc ...

  3. Specify where to find the sources, as an argument to `config.gcc':

          ../gcc-1.36/config.gcc -srcdir=../gcc-1.36 sun3

     The `-srcdir=DIR' option is not needed when the source directory
     is the parent of the current directory, because `config.gcc'
     detects that case automatically.

   Now, you can run `make' in that directory.  You need not repeat the
configuration steps shown above, when ordinary source files change.  You
must, however, run `config.gcc' again when the configuration files
change, if your system does not support symbolic links.


File: gcc.info,  Node: Sun Install,  Next: 3b1 Install,  Prev: Other Dir,  Up: Installation

Installing GNU CC on the Sun
============================

   Make sure the environment variable `FLOAT_OPTION' is not set when
you compile `gnulib'.  If this option were set to `f68881' when
`gnulib' is compiled, the resulting code would demand to be linked with
a special startup file and would not link properly without special
pains.

   There is a bug in `alloca' in certain versions of the Sun library.
To avoid this bug, install the binaries of GNU CC that were compiled by
GNU CC.  They use `alloca' as a built-in function and never the one in
the library.

   Some versions of the Sun compiler crash when compiling GNU CC, with a
segmentation fault in cpp.  This can sometimes be due to the bulk of
data in the environment variables.  You may be able to avoid it by using
the following command to compile GNU CC with Sun CC:

     make CC="TERMCAP=x OBJS=x LIBFUNCS=x STAGESTUFF=x cc"

   Another problem that often happens on Suns is that you get a crash
when building stage 2, when `genflags' is run.

   One reason for such as crash is if you configured GNU CC for the
wrong version of SunOS.  Starting with version 1.38, configurations
`sun3' and `sun4' are for SunOS 4, so this problem should no longer
happen.

   Another cause of the same symptom is having installed the GNU linker
with an earlier version of SunOS.  The version that worked before
stopped working due to a change in the format of executables in SunOS
4.1.  Many sites have installed the GNU linker as
`/usr/local/lib/gcc-ld', often as part of installing GNU C++.  So if
you get such crashes and you have used the proper configuration, try
deleting `/usr/local/lib/gcc-ld'.

   The current version of the GNU linker, found in the current binutils
release, does work with SunOS 4.1.


File: gcc.info,  Node: 3b1 Install,  Next: SCO Install,  Prev: Sun Install,  Up: Installation

Installing GNU CC on the 3b1
============================

   Installing GNU CC on the 3b1 is difficult if you do not already have
GNU CC running, due to bugs in the installed C compiler.  However, the
following procedure might work.  We are unable to test it.

  1. Comment out the `#include "config.h"' line on line 37 of `cccp.c'
     and do `make cpp'.  This makes a preliminary version of GNU cpp.

  2. Save the old `/lib/cpp' and copy the preliminary GNU cpp to that
     file name.

  3. Undo your change in `cccp.c', or reinstall the original version,
     and do `make cpp' again.

  4. Copy this final version of GNU cpp into `/lib/cpp'.

  5. Replace every occurrence of `obstack_free' in `tree.c' with
     `_obstack_free'.

  6. Run `make' to get the first-stage GNU CC.

  7. Reinstall the original version of `/lib/cpp'.

  8. Now you can compile GNU CC with itself and install it in the normal
     fashion.

   If you have installed an earlier version of GCC, you can compile the
newer version with that.  However, you will run into trouble compiling
`gnulib', since that is normally compiled with CC.  To solve the
problem, uncomment this line in `Makefile':

     CCLIBFLAGS = -B/usr/local/lib/gcc- -tp -Wp,-traditional


File: gcc.info,  Node: SCO Install,  Next: VMS Install,  Prev: 3B1 Install,  Up: Installation

Installing GNU CC on SCO System V 3.2
=====================================

   The compiler that comes with this system does not work properly with
`-O'.  Therefore, you should redefine the Make variable `CCLIBFLAGS'
not to use `-O'.

   You should also edit `Makefile' to enable the lines that set `CLIB'
to `-lPW', and the ones specifically labeled as being for SCO, that set
`RANLIB', and that set `CC' and `OLDCC' to `rcc -Di386 -DM_UNIX
-DM_I386 -DM_SYSV -DM_COFF'.

   Also, edit the definition of `USER_H' to remove the file `limits.h'.

   Then you can run `config.gcc i386-sco' and finish building GNU CC
normally.

   Note that the function `memmove' is broken in 3.2v2; it clobbers
register `%ebx'.  See the file `sco-memmove.s'.

   The same recipe should work on ESIX, but use `config.gcc i386-esix'
instead.


File: gcc.info,  Node: VMS Install,  Next: HPUX Install,  Prev: SCO Install,  Up: Installation

Installing GNU CC on VMS
========================

   The VMS version of GNU CC is distributed in a backup saveset
containing both source code and precompiled binaries.

   To install the `gcc' command so you can use the compiler easily, in
the same manner as you use the VMS C compiler, you must install the VMS
CLD file for GNU CC as follows:

  1. Define the VMS logical names `GNU_CC' and `GNU_CC_INCLUDE' to
     point to the directories where the GNU CC executables (`gcc-cpp',
     `gcc-cc1', etc.) and the C include files are kept.  This should be
     done with the commands:

          $ assign /super /system disk:[gcc.] gnu_cc
          $ assign /super /system disk:[gcc.include.] gnu_cc_include

     with the appropriate disk and directory names.  These commands can
     be placed in your system startup file so they will be executed
     whenever the machine is rebooted.  You may, if you choose, do this
     via the `GCC_INSTALL.COM' script in the `[GCC]' directory.

  2. Install the `GCC' command with the command line:

          $ set command /table=sys$library:dcltables gnu_cc:[000000]gcc

  3. To install the help file, do the following:

          $ lib/help sys$library:helplib.hlb gcc.hlp

     Now you can invoke the compiler with a command like `gcc /verbose
     file.c', which is equivalent to the command `gcc -v -c file.c' in
     Unix.

   We try to put corresponding binaries and sources on the VMS
distribution tape.  But sometimes the binaries will be from an older
version that the sources, because we don't always have time to update
them.  (Use the `/verbose' option to determine the version number of
the binaries and compare it with the source file `version.c' to tell
whether this is so.)  In this case, you should use the binaries you get
to recompile the sources.  If you must recompile, here is how:

  1. Copy the file `tm-vms.h' to `tm.h', `xm-vms.h' to `config.h',
     `vax.md' to `md.' and `out-vax.c' to `aux-output.c'.  The files to
     be copied are found in the subdirectory named `config'; they
     should be copied to the main directory of GNU CC.

  2. Setup the logical names and command tables as defined above.  In
     addition, define the vms logical name `GNU_BISON' to point at the
     to the directories where the Bison executable is kept.  This
     should be done with the command:

          $ assign /super /system disk:[bison.] gnu_bison

     You may, if you choose, use the `INSTALL_BISON.COM' script in the
     `[BISON]' directory.

  3. Install the `BISON' command with the command line:

          $ set command /table=sys$library:dcltables gnu_bison:[000000]bison

  4. Type `@make' to do recompile everything.

     If you are compiling with a version of GNU CC older than 1.33,
     specify `/DEFINE=("inline=")' as an option in all the
     compilations.  This requires editing all the `gcc' commands in
     `make-cc1.com'. (The older versions had problems supporting
     `inline'.)  Once you have a working 1.33 or newer GNU CC, you can
     change this file back.

   Due to the differences between the filesystems of Unix and VMS, the
preprocessor attempts to translate the names of include files into
something that VMS will understand.  The basic strategy is to prepend a
prefix to the specification of the include file, convert the whole
filename to a VMS filename, and then try to open the file.  The
preprocessor tries various prefixes until one of them succeeds.

   The first prefix is the `GNU_CC_INCLUDE:' logical name: this is
where GNU_C header files are traditionally stored.  If a header file is
not found there, `SYS$SYSROOT:[SYSLIB.]' is tried next.  If the
preprocessor is still unable to locate the file, it then assumes that
the include file specification is a valid VMS filename all by itself,
and it uses this filename to attempt to open the include file.  If none
of these strategies succeeds, the preprocessor reports an error.

   If you wish to store header files in non-standard locations, then you
can assign the logical `GNU_CC_INCLUDE' to be a search list, where each
element of the list is suitable for use with a rooted logical.

   With this version of GNU CC, `const' global variables now work
properly.  Unless, however, the `const' modifier is also specified in
every external declaration of the variable in all of the source files
that use that variable, the linker will issue warnings about conflicting
attributes for the variable, since the linker does not know if the
variable should be read-only.  The program will still work, but the
variable will be placed in writable storage.

   Due to an assembler bug, offsets to static constants are sometimes
incorrectly evaluated.  This bug is present in GAS 1.38.1, and should be
fixed in the next version.

   Under previous versions of GNU CC, the generated code would
occasionally give strange results when linked to the sharable `VAXCRTL'
library. Now this should work.

   Even with this version, however, GNU CC itself should not be linked
to the sharable `VAXCRTL'. The `qsort' routine supplied with `VAXCRTL'
has a bug which can cause a compiler crash.

   Similarly, the preprocessor should not be linked to the sharable
`VAXCRTL'. The `strncat' routine supplied with `VAXCRTL' has a bug
which can cause the preprocessor to go into an infinite loop.

   It should be pointed out that if you attempt to link to the sharable
`VAXCRTL', the VMS linker will strongly resist any effort to force it
to use the `qsort' and `strncat' routines from `gcclib'.  Until the
bugs in `VAXCRTL' have been fixed, linking any of the compiler
components to the sharable VAXCRTL is not recommended.  (These routines
can be bypassed by placing duplicate copies of `qsort' and `strncat' in
`gcclib' under different names, and patching the compiler sources to
use these routines).  Both of the bugs in `VAXCRTL' are still present
in VMS version 5.4-1, which is the most recent version as of this
writing.

   The executables that are generated by `make-cc1.com' and
`make-cccp.com' use the non-shared version of `VAXCRTL' (and thus use
the `qsort' and `strncat' routines from `gcclib.olb').

   Note that GNU CC on VMS now generates debugging information to
describe the programs symbols to the VMS debugger.  However, you need
version 1.37 or later of GAS in order to output them properly in the
object file.

   The VMS linker does not distinguish between upper and lower case
letters in function and variable names.  However, usual practice in C
is to distinguish case.  Normally GNU C (by means of the assembler GAS)
implements usual C behavior by augmenting each name that is not all
lower-case.  A name is augmented by truncating it to at most 23
characters and then adding more characters at the end which encode the
case pattern the rest.

   Name augmentation yields bad results for programs that use
precompiled libraries (such as Xlib) which were generated by another
compiler.  Use the compiler option `/NOCASE_HACK' to inhibits
augmentation; it makes external C functions and variables
case-independent as is usual on VMS.  Alternatively, you could write
all references to the functions and variables in such libraries using
lower case; this will work on VMS, but is not portable to other
systems.  In cases where you need to selectively inhibit augmentation,
you can define a macro for each mixed case symbol for which you wish to
inhibit augmentation, where the macro expands into the lower case
equivalent of the name.


File: gcc.info,  Node: HPUX Install,  Next: Tower Install,  Prev: VMS Install,  Up: Installation

Installing GNU CC on HPUX
=========================

   To install GNU CC on HPUX, you must start by editing the file
`Makefile'.  Search for the string `HPUX' to find comments saying what
to change.  You need to change some variable definitions and (if you
are using GAS) some lines in the rule for the target `gnulib'.

   To avoid errors when linking programs with `-g', create an empty
library named `libg.a'.  An easy way to do this is:

     ar rc /usr/local/lib/libg.a

   To compile with the HPUX C compiler, you must specify get the file
`alloca.c' from GNU Emacs.  Then, when you run `make', use this
argument:

     make ALLOCA=alloca.o

   When recompiling GNU CC with itself, do not define `ALLOCA'.
Instead, an `-I' option needs to be added to `CFLAGS' as follows:

     make CC=stage1/gcc CFLAGS="-g -O -Bstage1/ -I../binutils/hp-include"


File: gcc.info,  Node: Tower Install,  Prev: HPUX Install,  Up: Installation

Installing GNU CC on an NCR Tower
=================================

   On an NCR Tower model 4x0 or 6x0, you may have trouble because the
default maximum virtual address size of a process is just 1 Mb.  Most
often you will find this problem while compiling GNU CC with itself.

   The only way to solve the problem is to reconfigure the kernel. Add
a line such as this to the configuration file:

     MAXUMEM = 4096

and then relink the kernel and reboot the machine.
